**Title:** L/HIRF Terminology

**Submitter: Embraer (LHWG accepted)**

**Issue:** Use of term “L/HIRF Protection System” in new MSG-3 L/HIRF logic needs to be deleted since it is no longer referred to in the MSG-3 Rev 2013.1 .

**Problem:** New logic does not refer to L/HIRF protection systems. Definition of L/HIRF Protection System is listed in the Appendix A. Glossary and is not required since it is no longer referred to in the L/HIRF Analysis Procedure section - MSG-3 Rev. 2013.1.

**Recommendation (including Implementation):**

To delete the term “L/HIRF Protection System” from the Appendix A. Glossary *(page 82 - ATA MSG-3 Volume 1)*

L/HIRF Protection Components Any self-contained part, combination of

parts, subassemblies, units, or structures

that perform a distinctive function necessary

to provide L/HIRF protection.

.

**IMRBPB Position:**

**Date:**

**Position:.**

**Status of Issue Paper (when closed state the closure date):**

**Recommendation for implementation:**

**Important Note:** The IMRBPB positions are not policy. Positions become policy only when the policy is issued formally by the appropriate National Aviation Authority.